HTTP

Web pages:

MPFS is defined space in ROM and the image is created with MPFS2.JAR

HTML written as always

Javascript MCHP.Js handles the handshaking between client’s web browser and http server.

There some .xml dynamic variables?

There is some .cgi dynamic variables?

http serves up (parses) a web page from the MPFS rom configured files. When it encounters a .cgi file and a ~variable~ it calls the http print variable function and makes a replacement to the html it serves up. Dynamic variables.