WiFi Sensor V1.2

Dimension: 3.1”x1.75”/(78.7mm x 44.4mm)

Two Layer board

Thickness: ~.062”/~(1.57mm)

Parts: ~78-surface mount 0-through hole parts loaded

Colors : no preference